Physical Coding Sublayer (PCS): Encoding the binary data from layer 2

Physical Medium Attachment (PMA): Parallel to serial and in constrast

Physical Medium Dependent (PMD): Voltage amplififes/LEDs/Lasers