**REVIEW**

Q.1) Two protocols are supported on Cisco devices for AAA communications are **RADIUS (Remote Authentication Dial-In User Service) and TACAS+ (Terminal Access Controller Access-Control System Plus).**

Q.2) **CDP (Cisco Discovery Protocol)** is enabled on a Cisco router by default that can reveal significant information about the router and potentially make it more vulnerable to attack.

Q.3) When security is a concern, **Layer 2** is considered to be the weakest link in a network system